{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"merged":[[0,0,0,5]],"flags":["formulas_cached_only"]}
["淖尔壕煤矿智能化建设第二阶段设备采购清单（公开招标部分）"]
["序号","设备材料名称","型号","单位","数量","备注"]
["标段一","煤溜监测系统","1、智能煤流节能调速系统\n2、输送带探伤装置\n3、远程控制台","套",1,"详见技术规格书"]
["标段二","通风监测系统","1、矿井通风参数智能感知子系统\n2、矿井高效全自动测风子系统\n3、风量远程定量调控子系统\n4、风门自动化调控\n5、三维矿井通风智能分析决策平台\n6、局部通风子系统（含3套6台风机）","套",1,"详见技术规格书，局部通风机为变频通风机"]
["标段三","光纤测温系统","一、光纤测温\n1、测温范围：-10℃—120℃\n2、单通道最大测量距离：≥6km\n3、测温精度：±1℃\n4、定位精度：±1m\n5、通讯接口：以太网/光口/电口\n6、通道数量：满足配置要求，并至少预留2路备用\n7、监测范围：采空区、主运沿线、井下变电所电缆沟槽\n8、地面布置监控主备机，具有实时显示、图形显示、曲线显示、报表查询等功能。\n二、地面变电所自动防灭火系统\n1、喷射距离：≥2m。\n2、采用热敏线探测，传导速度不低于3米/秒。\n3、自动启动温度为70\n4、场所范围：主通风机房配电室（96㎡）、主井机头房高压配电室（96㎡）；35KV变电站（2320㎡）、锅炉房配电室（面积150㎡）","套",1,"详见技术规格书"]
["标段四","矿压监测系统","1、传感器采用无线传输方式，自组网通信\n2、井上下数据传输距离不低于20km\n3、监测范围：1409工作面两顺槽","套",1,"详见技术规格书"]
["标段五","探放水系统","1、系统包括服务平台、感知应用平台和智能终端平台。\n2、可实现煤矿探放水钻孔施工过程中钻孔设计、钻孔任务、钻孔作业（井下作业APP）、钻孔验收、钻孔台帐、巡检作业、达标评判等全过程信息化管理。\n3、系统应用人工智能视频识别技术分析探水视频，自动计算钻孔深度，同时通过井下APP拍摄上传钻孔角度图像，保障钻孔到位，有效杜绝谎报进尺、违章操作、打假孔等危及安全的事件发生。","套",1,"详见技术规格书"]
["标段六","智能化掘锚机","1、型号：EBZ200M\n2、掘锚机集成掘进、临时支护、锚杆的功能，机载2个锚杆钻机，1个临时支护。\n3、掘进机配套带式输送机用自移机尾、第二运输机、除尘系统、自动张紧装置。\n4、掘进机具有远程智能控制系统，具有智能控制系统、可视化系统、传感系统及软件系统等子系统。可接入井下5G通信网络。","套",1,"详见技术规格书"]
["标段七","矿用液压移动列车组",null,"套",1]
[1,"泵站",null,"套",1,"含液箱"]
[2,"矿用液压移动列车组单车","长度4000，宽度1400","台",28,"详见技术规格书"]
[3,"矿用液压移动列车组单车","长度4500，宽度1400","台",4,"详见技术规格书"]
[4,"矿用液压移动列车组单车","长度6000，宽度1400","台",3,"详见技术规格书"]
["标段八","综采工作面电缆"]
[1,"采煤机电缆","MCPTJX-1.9/3.3 3×150+3×70/3+3×(2×2.5)","米",560,"采煤机电缆型号仅供参考实际型号已各投标厂家为准。"]
[2,"刮板输送机电缆","MCPT-1.9/3.3KV 3*70+1*35+3*4","米",840]
[3,"转载机电缆/破碎机电缆","MYP-0.66/1.14KV 3*120+1*35","米",480]
[4,"高压电缆","MYPTJ-8.7/10KV3*150+3*50/3+3*2.5","米",2500]
[5,"高压电缆","MYPTJ-8.7/10KV3*50+3*25/3+3*2.5","米",2500]
[6,"低压电缆","MYP-0.66/1.14KV 3*25+1*16","米",500]
["标段九","综采顺槽胶带机带面","PVG1800S","米",3000,"详见技术规格书"]
["标段十","馈电、组合开关及照明综保"]
[1,"馈电开关","KBZ-400/1140（660）","台",5,"带标准485通讯接口"]
[2,"馈电开关","KBZ-200/1140（660）","台",4,"带标准485通讯接口"]
[3,"组合开关","QJZ-8*80/1140（600）","台",2,"带标准485通讯接口"]
[4,"综保","ZBZ-6.0/1140(660)/127","台",2,"带标准485通讯接口"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}